867 Product Transfer and Resale Report

Functional Group ID=PT

Introduction:

This Draft Standard for Trial Use contains the format and establishes the data contents of the Product Transfer and Resale Report Transaction Set (867) for use within the context of an Electronic Data Interchange (EDI) environment. The transaction set can be used to: (1) report information about product that has been transferred from one location to another; (2) report sales of product from one or more locations to an end customer; or (3) report sales of a product from one or more locations to an end customer, and demand beyond actual sales (lost orders). Report may be issued by either buyer or seller.

Notes:

Heading:

	Pos.	Seg.		Req.		Loop	Notes and
	No.	ID	Name	Des.	Max.Use	Repeat	Comments	
M	010	ST	Transaction Set Header	M	1									
M	020	BPT	Beginning Segment for Product Transfer and Resale	M	1									
	050	DTM	Date/Time Reference (Document Due Date)	O	10									
	060	REF	Reference Identification (Customer Account ID or SDID)	O	12									
	060	REF	Reference Identification (Non-Billing Party Account ID)	O	12									
	060	REF	Reference Identification (Billing Party Old Account ID)	O	12									
	060	REF	Reference Identification(Original Usage Unique ID)	O	12									
	060	REF	Reference Identification(Party Sending Bill)	O	12									
	060	REF	Reference Identification(Party Calculating Non-Billing Party Charges)	O	12									
	060	REF	Reference Identification(Power Region)	O	12									
			LOOP ID - N1			5								
	080	N1	Name (Distribution Company)	O	1									
														
			LOOP ID - N1			5								
	080	N1	Name (Registration Agent)	O	1									
														
			LOOP ID - N1			5								
	080	N1	Name (Supplier)	O	1									

Detail:

	Pos.	Seg.		Req.		Loop	Notes and
	No.	ID	Name	Des.	Max.Use	Repeat	Comments	
			LOOP ID - PTD			>1								
M	010	PTD	Product Transfer and Resale Detail (Monthly Billed Summary)	M	1									
	020	DTM	Date/Time Reference (Service Period Start)	O	10									
	020	DTM	Date/Time Reference (Service Period End)	O	10									
			LOOP ID - QTY			>1								
	110	QTY	Quantity {Billed KWH)	O	1									
														
			LOOP ID - QTY			>1								
	110	QTY	Quantity {Billed Demand)	O	1									
														
			LOOP ID - QTY			>1								
	110	QTY	Quantity {Measured Demand)	O	1									
														
			LOOP ID - PTD			>1								
M	010	PTD	Product Transfer and Resale Detail (Non-Interval Detail)	M	1									
	020	DTM	Date/Time Reference (Service Period Start)	O	10									
	020	DTM	Date/Time Reference (Service Period End)	O	10									
	020	DTM	Date/Time Reference (Exchange Date)	O	10									
	030	REF	Reference Identification (Number of Dials)	O	>1									
	030	REF	Reference Identification (Meter Role)	O	20									
	030	REF	Reference Identification (Meter Type)	O	20									
			LOOP ID - QTY			>1								
	110	QTY	Quantity	O	1									
	160	MEA	Measurements (Meter Reads)	O	40									
	160	MEA	Measurements (Transformer Loss Factor)	O	40									
	160	MEA	Measurements (Meter Multiplier)	O	40									
	160	MEA	Measurements (Power Factor)	O	40									
														
			LOOP ID - PTD			>1								
M	010	PTD	Product Transfer and Resale Detail (Unmetered Services)	M	1									
	020	DTM	Date/Time Reference (Service Period Start)	O	10									
	020	DTM	Date/Time Reference (Service Period End)	O	10									
	030	REF	Reference Identification (Unmetered Service Type)	O	20									
			LOOP ID - QTY			>1								
	110	QTY	Quantity	O	1									
														
			LOOP ID - PTD			>1								
M	010	PTD	Product Transfer and Resale Detail (Interval Summary)	M	1									
	020	DTM	Date/Time Reference (Service Period Start)	O	10									
	020	DTM	Date/Time Reference (Service Period End)	O	10									
	020	DTM	Date/Time Reference (Exchange Date)	O	10									
	030	REF	Reference Identification (Meter Role)	O	20									
	030	REF	Reference Identification (Meter Type)	O	20									
			LOOP ID - QTY			>1								
	110	QTY	Quantity	O	1									
	160	MEA	Measurements (Meter Reads)	O	40									
	160	MEA	Measurements (Transformer Loss Factor)	O	40									
	160	MEA	Measurements (Meter Multiplier)	O	40									
	160	MEA	Measurements (Power Factor)	O	40									
														
			LOOP ID - PTD			>1								
M	010	PTD	Product Transfer and Resale Detail (Interval Detail)	M	1									
	020	DTM	Date/Time Reference (Service Period Start)	O	10									
	020	DTM	Date/Time Reference (Service Period End)	O	10									
	020	DTM	Date/Time Reference (Exchange Date)	O	10									
	030	REF	Reference Identification (Channel Number)	O	20									
	030	REF	Reference Identification (Meter Type)	O	20									
	030	REF	Reference Identification (Meter Role)	O	20									
			LOOP ID - QTY			>1								
	110	QTY	Quantity	O	1									
	210	DTM	Date/Time Reference (Interval End Time)	O	10									

Summary:

	Pos.	Seg.		Req.		Loop	Notes and
	No.	ID	Name	Des.	Max.Use	Repeat	Comments	
M	030	SE	Transaction Set Trailer	M	1									

	Segment:	ST Transaction Set Header
	Position:	010
	Loop:
	Level:	Heading
	Usage:	Mandatory
	Max Use:	1
	Purpose:	To indicate the start of a transaction set and to assign a control number
	Syntax Notes:
	Semantic Notes:	1	The transaction set identifier (ST01) is used by the translation routines of the interchange partners to select the appropriate transaction set definition (e.g., 810 selects the Invoice Transaction Set).
	Comments:
Notes:		Required
	
		ST~867~000000001	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	ST01	143	Transaction Set Identifier Code	M		ID 3/3	
	Code uniquely identifying a Transaction Set	
 	867		Product Transfer and Resale Report	
Must Use	ST02	329	Transaction Set Control Number	M		AN 4/9	
	Identifying control number that must be unique within the transaction set functional group assigned by the originator for a transaction set	

	Segment:	BPT Beginning Segment for Product Transfer and Resale
	Position:	020
	Loop:
	Level:	Heading
	Usage:	Mandatory
	Max Use:	1
	Purpose:	To indicate the beginning of the Product Transfer and Resale Report Transaction Set and transmit identifying data
	Syntax Notes:	1	If either BPT05 or BPT06 is present, then the other is required.
	Semantic Notes:	1	BPT02 identifies the transfer/resale number.
		2	BPT03 identifies the transfer/resale date.
		3	BPT08 identifies the transfer/resale time.
		4	BPT09 is used when it is necessary to reference a Previous Report Number.
	Comments:
Notes:		Required
	
		BPT~00~200102010001~20010131~DD
BPT~00~200102010001~20010131~DD~~~F
BPT~01~200102020001~20010131~DD~~~~~2001020100001

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	BPT01	353	Transaction Set Purpose Code	M		ID 2/2	
	Code identifying purpose of transaction set	
 	00		Original	
	Conveys original readings for the account being reported.  If usage is canceled and restated, the restatement is sent as an original.	
 	01		Cancellation	
	Readings previously reported for the account are to be ignored.  This would cancel the entire period of usage for the period.	
Must Use	BPT02	127	Reference Identification	O		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	A unique transaction identification number assigned by the originator of this transaction.  This number must be unique over time.

Transaction Reference numbers will only contain uppercase letters (A to Z) and digits (0 to 9).  Note that punctuation (spaces, dashes, etc.) must be excluded.	
Must Use	BPT03	373	Date	M		DT 8/8	
	Date expressed as CCYYMMDD	
	The transaction creation date - the date that the data was processed by the sender's application system.	
Must Use	BPT04	755	Report Type Code	O		ID 2/2	
	Code indicating the title or contents of a document, report or supporting item	
 	C1		Cost Data Summary	
	Interval Meters	
 	DD		Distributor Inventory Report	
	Non-interval metered and unmetered	
 	DR		Datalog Report	
	Mixed Usage - both Interval and Non-interval Meters on account.	
Dep	BPT07	306	Action Code	O		ID 1/2	
	Code indicating type of action	
	Required for Final Usage Statement	
 	F		Final	
	Final meter read data being sent for this customer.  The customer account is final with the Distribution company or the customer switched to a new Energy Supplier.	
Dep	BPT09	127	Reference Identification	O		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	When BPT01 = 01 (cancel), this element is required and contains the transaction identification number from BPT02 of the transaction that is being cancelled.

Condition:  Required if a cancellation.	

	Segment:	DTM Date/Time Reference (Document Due Date)
	Position:	050
	Loop:
	Level:	Heading
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		Required for Consolidated Bill Ready Original Transactions
	
		Required for Bill Ready Consolidated Billing  where the meter reading party  sends an 867 to the non-billing party, who calculates their own portion of the bill and sends the 810 to the billing party. 

If a file is received by the Billing Party after the date and time specified in the DTM~649, and the Billing Party cannot process it for display on the current month's bill, the Billling Party must notify the Supplier via the 824(Application Advice) whether the Billing Party will reject the file and require the Supplier to resend next month or whether the Billing Party will hold the billing file for display on next month's bill without requiring the Supplier to resend.
	
		DTM~649~20020131~1800	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	649		Document Due	
	The date that the non-billing party must provide the 810 transaction back to the billing party.	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	
Must Use	DTM03	337	Time	X		TM 4/8	
	Time expressed in 24-hour clock time as follows: HHMM, or HHMMSS, or HHMMSSD, or HHMMSSDD, where H = hours (00-23), M = minutes (00-59), S = integer seconds (00-59) and DD = decimal seconds; decimal seconds are expressed as follows: D = tenths (0-9) and DD = hundredths (00-99)	
	HHMM, where H = Hours (00-23) and M = Minutes (00-59) in prevailing time at the meter controls.  For this transaction, since X12 does not allow 2400 for time, 2359 will be used to indicate midnight.  For example, midnight between October 15th and October 16th will be reflected as 2359 of October 15th.	

	Segment:	REF Reference Identification (Customer Account ID or SDID)
	Position:	060
	Loop:
	Level:	Heading
	Usage:	Optional
	Max Use:	12
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		Conditional on Governing Documents. Either REF~12 or REF~Q5 is required.	
		REF~12~10111111234567890ABCDEFGHIJKL
REF~Q5~~10111111234567890ABCDEFGHIJKL

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	12		Billing Account	
	Account number under which billing is rendered	
	Distribution Company assigned account number for the customer sent in REF02	
 	Q5		Property Control Number	
	Customer SDID - sent in REF03.	
Used	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	Customer Account ID - use when REF01 = 12.	
	This free-form text can not contain  any characters that may be used as element delimiters, sub-element delimiters, segment terminators, or field separators(This includes: asterisk *, pipes |, tabs, linefeeds, carets ^, angle brackets < >, and tildes ~).	
Must Use	REF03	352	Description	X		AN 1/80	
	A free-form description to clarify the related data elements and their content	
	Customer SDID - use when REF01 = Q5.	
	This free-form text can not contain  any characters that may be used as element delimiters, sub-element delimiters, segment terminators, or field separators(This includes: asterisk *, pipes |, tabs, linefeeds, carets ^, angle brackets < >, and tildes ~).	

	Segment:	REF Reference Identification (Non-Billing Party Account ID)
	Position:	060
	Loop:
	Level:	Heading
	Usage:	Optional
	Max Use:	12
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		RBC	
		REF~11~123456789019990102	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	11		Account Number	
	Number identifies a telecommunications industry account	
	Customer Account ID assigned by Non-Billing Party.	
Used	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	Customer Account ID assigned by Non-Billing Party.	

	Segment:	REF Reference Identification (Billing Party Old Account ID)
	Position:	060
	Loop:
	Level:	Heading
	Usage:	Optional
	Max Use:	12
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		RBC	
		Required if Account Number has changed in last 45 days	
		REF~45~212345438756

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	45		Old Account Number	
	Identifies accounts being changed	
	Previous Distribution Company assigned account number for end use customer.	
Must Use	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	Billing Party Old Account ID	
	ERCOT          Electric Reliability Council of Texas
SERC          Southeast Electric Reliability Council
SPP          Southwest Power Pool
WSCC          Western States Coordinating Council	

	Segment:	REF Reference Identification(Original Usage Unique ID)
	Position:	060
	Loop:
	Level:	Heading
	Usage:	Optional
	Max Use:	12
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		RBC, required on Final Usage, otherwise Not Used.

The source of this value will be the BGN06 of the Enrollmnent or Drop 814 Transactions sent from the Distribution Company to the Registration Agent.
	
		REF~TN~1234567820010620	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	TN		Transaction Reference Number	
	Usage Unique ID	
Must Use	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	The number that is tracked in the BGN06 through the lifecycle of the respective process.

	Segment:	REF Reference Identification(Party Sending Bill)
	Position:	060
	Loop:
	Level:	Heading
	Usage:	Optional
	Max Use:	12
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		Required	
		REF~BLT~LDC	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	BLT		Billing Type	
	Identifies the party sending the bill	
Must Use	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	When REF01 is BLT, valid values for REF02 are:
LDC (meaning the distribution company sends the bill to the customer)
ESP (meaning the suppliers sends the bill to the customer)
DUAL (meaning each party sends a bill to the customer)	

	Segment:	REF Reference Identification(Party Calculating Non-Billing Party Charges)
	Position:	060
	Loop:
	Level:	Heading
	Usage:	Optional
	Max Use:	12
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		Required	
		REF~PC~DUAL	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	PC		Production Code	
	Identifies the party that calculates the Non-Billing Party charges.	
Must Use	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	When REF01 is PC, valid values for REF02 are:
LDC (meaning the distribution company calculates the charges on the bill)
DUAL (meaning each party calculates their own portion of the charges)	

	Segment:	REF Reference Identification(Power Region)
	Position:	060
	Loop:
	Level:	Heading
	Usage:	Optional
	Max Use:	12
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		RBC	
		REF~SR~ERCOT   
REF~SR~SERC       
REF~SR~SPP            
REF~SR~WSCC            

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	SR		Sales Responsibility	
	Power Region	
Must Use	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	Power Region of the SDID
	
	ERCOT    Electric Reliability Council of Texas
SERC       Southweat Electric Reliability Council
SPP          Southwest Power Pool
WSCC       Western States Coordinating Council	

	Segment:	N1 Name (Distribution Company)
	Position:	080
	Loop:	N1        Optional
	Level:	Heading
	Usage:	Optional
	Max Use:	1
	Purpose:	To identify a party by type of organization, name, and code
	Syntax Notes:	1	At least one of N102 or N103 is required.
		2	If either N103 or N104 is present, then the other is required.
	Semantic Notes:
	Comments:	1	This segment, used alone, provides the most efficient method of providing organizational identification. To obtain this efficiency the "ID Code" (N104) must provide a key to the table maintained by the transaction processing party.
		2	N105 and N106 further define the type of entity in N101.
Notes:		Required
	
		N1~8S~DISCO LTD~1~007909411~~41 (Distribution Company to the Registration Agent)
N1~8S~DISCO LTD~1~007909411 (Registration Agent to the Supplier)	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	N101	98	Entity Identifier Code	M		ID 2/3	
	Code identifying an organizational entity, a physical location, property or an individual	
 	8S		Consumer Service Provider (CSP)	
	Distribution Company	
Must Use	N102	93	Name	X		AN 1/60	
	Free-form name	
	Distribution Company Name	
	This free-form text can not contain any characters that may be used as element delimiters, sub-element delimiters, segment terminators, or field separators.  (This includes: asterisk *, pipes |, tabs, linefeeds, carets ^, angle brackets < >, and tildes ~).	
Must Use	N103	66	Identification Code Qualifier	X		ID 1/2	
	Code designating the system/method of code structure used for Identification Code (67)	
 	1		D-U-N-S Number, Dun & Bradstreet	
 	9		D-U-N-S+4, D-U-N-S Number with Four Character Suffix	
Must Use	N104	67	Identification Code	X		AN 2/80	
	Code identifying a party or other code	
	Distribution Company Common Code Identifier	
Dep	N106	98	Entity Identifier Code	O		ID 2/3	
	Code identifying an organizational entity, a physical location, property or an individual	
 	41		Submitter	

	Segment:	N1 Name (Registration Agent)
	Position:	080
	Loop:	N1        Optional
	Level:	Heading
	Usage:	Optional
	Max Use:	1
	Purpose:	To identify a party by type of organization, name, and code
	Syntax Notes:	1	At least one of N102 or N103 is required.
		2	If either N103 or N104 is present, then the other is required.
	Semantic Notes:
	Comments:	1	This segment, used alone, provides the most efficient method of providing organizational identification. To obtain this efficiency the "ID Code" (N104) must provide a key to the table maintained by the transaction processing party.
		2	N105 and N106 further define the type of entity in N101.
Notes:		RBC
	
		N1~AY~RA~1~888777888~~40 (Distribution Company to the Registration Agent)
N1~AY~RA~1~888777888~~41 (Clearinghouse to the Registration Agent)	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	N101	98	Entity Identifier Code	M		ID 2/3	
	Code identifying an organizational entity, a physical location, property or an individual	
 	AY		Clearinghouse	
	Registration Agent	
Must Use	N102	93	Name	X		AN 1/60	
	Free-form name	
	Registration Agent Name	
	This free-form text can not contain  any characters that may be used as element delimiters, sub-element delimiters, segment terminators, or field separators(This includes: asterisk *, pipes |, tabs, linefeeds, carets ^, angle brackets < >, and tildes ~).	
Must Use	N103	66	Identification Code Qualifier	X		ID 1/2	
	Code designating the system/method of code structure used for Identification Code (67)	
 	1		D-U-N-S Number, Dun & Bradstreet	
Must Use	N104	67	Identification Code	X		AN 2/80	
	Code identifying a party or other code	
	Registration Agent Common Code Identifier	
Must Use	N106	98	Entity Identifier Code	O		ID 2/3	
	Code identifying an organizational entity, a physical location, property or an individual	
 	40		Receiver	
 	41		Submitter	

	Segment:	N1 Name (Supplier)
	Position:	080
	Loop:	N1        Optional
	Level:	Heading
	Usage:	Optional
	Max Use:	1
	Purpose:	To identify a party by type of organization, name, and code
	Syntax Notes:	1	At least one of N102 or N103 is required.
		2	If either N103 or N104 is present, then the other is required.
	Semantic Notes:
	Comments:	1	This segment, used alone, provides the most efficient method of providing organizational identification. To obtain this efficiency the "ID Code" (N104) must provide a key to the table maintained by the transaction processing party.
		2	N105 and N106 further define the type of entity in N101.
Notes:		Required	
		N1~SJ~SUPPLY LTD~9~007909422CRN1 (Distribution Company to Registration Agent)
N1~SJ~SUPPLY LTD~9~007909422CRN1~~40 (Registration Agent to Supplier)	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	N101	98	Entity Identifier Code	M		ID 2/3	
	Code identifying an organizational entity, a physical location, property or an individual	
 	SJ		Service Provider	
	Supplier	
Must Use	N102	93	Name	X		AN 1/60	
	Free-form name	
	Supplier Name	
	This free-form text can not contain  any characters that may be used as element delimiters, sub-element delimiters, segment terminators, or field separators(This includes: asterisk *, pipes |, tabs, linefeeds, carets ^, angle brackets < >, and tildes ~).	
Must Use	N103	66	Identification Code Qualifier	X		ID 1/2	
	Code designating the system/method of code structure used for Identification Code (67)	
 	1		D-U-N-S Number, Dun & Bradstreet	
 	9		D-U-N-S+4, D-U-N-S Number with Four Character Suffix	
Must Use	N104	67	Identification Code	X		AN 2/80	
	Code identifying a party or other code	
	Supplier Common Code Identifier	
Dep	N106	98	Entity Identifier Code	O		ID 2/3	
	Code identifying an organizational entity, a physical location, property or an individual	
 	40		Receiver	

	Segment:	PTD Product Transfer and Resale Detail (Monthly Billed Summary)
	Position:	010
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Mandatory
	Max Use:	1
	Purpose:	To indicate the start of detail information relating to the transfer/resale of a product and provide identifying data
	Syntax Notes:	1	If either PTD02 or PTD03 is present, then the other is required.
		2	If either PTD04 or PTD05 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD Loops may be sent in any order.

One Monthly Billed Summary PTD loop is required for every account.	
		PTD~BB	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	PTD01	521	Product Transfer Type Code	M		ID 2/2	
	Code identifying the type of product transfer	
 	BB		Demand Information Only	
	No physical transfer of material occurs; historical demand information is provided for record purposes only	
	This information is obtained from the billing system to reflect the billing data for this account at the unit of measure level.	

	Segment:	DTM Date/Time Reference (Service Period Start)
	Position:	020
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		Required
	
		DTM~150~20050101	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	150		Service Period Start	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	

	Segment:	DTM Date/Time Reference (Service Period End)
	Position:	020
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		Required
	
		DTM~151~20050131	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	151		Service Period End	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	
	Date	

	Segment:	QTY Quantity {Billed KWH)
	Position:	110
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	1
	Purpose:	To specify quantity information
	Syntax Notes:	1	At least one of QTY02 or QTY04 is required.
		2	Only one of QTY02 or QTY04 may be present.
	Semantic Notes:	1	QTY04 is used when the quantity is non-numeric.
	Comments:
Notes:		Required	
		QTY~D1~22348~KH

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	QTY01	673	Quantity Qualifier	M		ID 2/2	
	Code specifying the type of quantity	
 	D1		Billed	
	Used when Quantity in QTY02 is a "Billed" quantity.	
Must Use	QTY02	380	Quantity	X		R 1/15	
	Numeric value of quantity	
Used	QTY03	C001	Composite Unit of Measure	O			
	To identify a composite unit of measure  (See Figures Appendix for examples of use)	
	Note this is a composite data element, populate C00101	
Must Use	C00101	355	Unit or Basis for Measurement Code	M		ID 2/2	
	Code specifying the units in which a value is being expressed, or manner in which a measurement has been taken	
 	KH		Kilowatt Hour	
	Billed kilowatt Hours as shown on the customer's bill.  May or may not be the same as measured kilowatt hours.	

	Segment:	QTY Quantity {Billed Demand)
	Position:	110
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	1
	Purpose:	To specify quantity information
	Syntax Notes:	1	At least one of QTY02 or QTY04 is required.
		2	Only one of QTY02 or QTY04 may be present.
	Semantic Notes:	1	QTY04 is used when the quantity is non-numeric.
	Comments:
Notes:		Required if account measures Demand (KW).  This must be sent even if Billed (derived) demand is equal to measured demand.	
		QTY~D1~22~K1

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	QTY01	673	Quantity Qualifier	M		ID 2/2	
	Code specifying the type of quantity	
 	D1		Billed	
	Used when Quantity in QTY02 is a "Billed" quantity.	
Must Use	QTY02	380	Quantity	X		R 1/15	
	Numeric value of quantity	
Used	QTY03	C001	Composite Unit of Measure	O			
	To identify a composite unit of measure  (See Figures Appendix for examples of use)	
	Note this is a composite data element, populate C00101	
Must Use	C00101	355	Unit or Basis for Measurement Code	M		ID 2/2	
	Code specifying the units in which a value is being expressed, or manner in which a measurement has been taken	
 	K1		Kilowatt Demand	
	kW	

	Segment:	QTY Quantity {Measured Demand)
	Position:	110
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	1
	Purpose:	To specify quantity information
	Syntax Notes:	1	At least one of QTY02 or QTY04 is required.
		2	Only one of QTY02 or QTY04 may be present.
	Semantic Notes:	1	QTY04 is used when the quantity is non-numeric.
	Comments:
Notes:		Required if account measures Demand (KW)	
		QTY~QD~14~K1

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	QTY01	673	Quantity Qualifier	M		ID 2/2	
	Code specifying the type of quantity	
 	KA		Estimated	
	Used when Quantity in QTY02 is Estimated.	
 	QD		Quantity Delivered	
	Used when Quantity in QTY02 is Actual	
Must Use	QTY02	380	Quantity	X		R 1/15	
	Numeric value of quantity	
Used	QTY03	C001	Composite Unit of Measure	O			
	To identify a composite unit of measure  (See Figures Appendix for examples of use)	
	Note this is a composite data element, populate C00101	
Must Use	C00101	355	Unit or Basis for Measurement Code	M		ID 2/2	
	Code specifying the units in which a value is being expressed, or manner in which a measurement has been taken	
 	K1		Kilowatt Demand	
	kW	

	Segment:	PTD Product Transfer and Resale Detail (Non-Interval Detail)
	Position:	010
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Mandatory
	Max Use:	1
	Purpose:	To indicate the start of detail information relating to the transfer/resale of a product and provide identifying data
	Syntax Notes:	1	If either PTD02 or PTD03 is present, then the other is required.
		2	If either PTD04 or PTD05 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = PL (Non-Interval Detail)
	
		There will be one PTD~PL loop for each meter for each unit of measure.  There will also be separate PTD~PL loops to reflect missing or abundance of consumption.

For Additive/Subtractive Metering Only:
This loop is also used to for Additive/Subtractive Metering when the Master Meter is on one ESI ID and the additive and/or subtractive meters are on ESI IDs that are different than the master Meter.   All additive usage is summed.  All subtractive usage is summed.  It is possible to receive two additive/subtractive loops - one with summed additive usage and one with summed subtractive usage.  When reporting usage for the additive/Master and/or subtractive/Master usage, the meter number is not provided in the PTD04 and PTD05.  The type of Master/Additive/Subtractive usage must be provided in the PTD06 by using code "AI" or code "AO".

For Missing or Abundance of Consumption  - Non Interval:
This loop is also used to report missing or abundance of consumption when the consumption (added or subtracted) provided has not been registered by the meter, for example: tampering, fast, slow and/or flat/bypass.  The conditions exist only for non-interval meters on the same ESI ID.  The meter number must be provided in the PTD04 and PTD05.  The type of missing or abundance consumption must be provided in the PTD06.  .  The receiver must add or subtract this consumption from the meter number provided in the PTD05.  Net usage for the ESI ID is provided in the PTD~SU Loop.	
		PTD~PL~~~MG~1234568MG
PTD~PL~~~~~AO (used to report subtractive metering off a master meter)
PTD~PL~~~MG~1234568MG~MD (used to report tampering)	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	PTD01	521	Product Transfer Type Code	M		ID 2/2	
	Code identifying the type of product transfer	
 	PL		Property Level Movement/Sale	
	Non-Interval Detail	
Dep	PTD04	128	Reference Identification Qualifier	X		ID 2/3	
	Code qualifying the Reference Identification	
 	MG		Meter Number	
	Not used if the PTD06= "AO" or "AI"	
Dep	PTD05	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	Meter Number

Meter numbers will contain only uppercase letters (A to Z) and digits (0 to 9).  Note that punctuation (spaces, dashes, etc.) must be excluded, and significant leading and trailing zeros that are part of the meter number must be present.

Not used if the PTD06= "AO" or "AI".
	
Used	PTD06	486	Product Transfer Movement Type Code	O		ID 2/2	
	To indicate the type of product transfer movement	
	RBC	
	To indicate the type of product transfer movement.  This field is only used when reporting the type of Master/Additive usage, Master/Subtractive usage or missing or abundance of consumption adjustment.  The receiver must add this consumption to the meter number provided in the PTD05.   	
 	AI		Adjustment In	
	Additive Metering

Additive Usage for Additive meters off the master meter where a different SDID has been assigned to the master and/or all applicable additive meters.  When the PTD06 equals "AI", the REF~JH equals "A". 	
 	AO		Adjustment Out	
	Subtractive Metering

Subtractive Usage for Subtract meters off the master meter where a different SDID has been assigned to the master and/or all applicable subtractive meters.  .  When the PTD06 equals "AO", the REF~JH equals "S".  	
 	CD		Customer to Distributor	
	Added Flat /Bypass - Missing or Abundance of Consumption

For adjusting consumption when the added consumption provided has not been registered by the meter.   The condition exists only for non-interval meters on the same SDID.  The receiver must add this consumption to the meter number provided in the PTD05.  The receiver must add this consumption to the meter number provided in the PTD05.  When the PTD06 equals "CD", the REF~JH equals "A".	
 	DC		Distributor to Customer	
	Added Slow- Missing or Abundance of Consumption

For adjusting consumption when the added consumption provided has not been registered by the meter.  The conditions exists only for non-interval meters on the same SDID.  The receiver must add this consumption to the meter number provided in the PTD05.  When the PTD06 equals "DC", the REF~JH equals "A".  	
 	DM		Distributor to Manufacturer	
	Subtracted Fast- Missing or Abundance of Consumption

For adjusting consumption when the subtracted consumption provided has not been registered by the meter.  The condition exists only for non-interval meters on the same SDID.  The receiver must subtract this consumption to the meter number provided in the PTD05.  When the PTD06 equals "DM", the REF~JH equals "S".  	
 	MD		Manufacturer to Distributor	
	Added Tampering- Missing or Abundance of Consumption

For adjusting consumption when the added consumption provided has not been registered by the meter.  The condition exists only for non-interval meters on the same SDID.  The receiver must add this consumption to the meter number provided in the PTD05.  When the PTD06 equals "MD", the REF~JH equals "A".  	

	Segment:	DTM Date/Time Reference (Service Period Start)
	Position:	020
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = PL (Non-Interval Detail)
	
		Required, unless an Exchange Date (DTM~514) is substituted for this code.
	
		DTM~150~20010101	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	150		Service Period Start	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	

	Segment:	DTM Date/Time Reference (Service Period End)
	Position:	020
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = PL (Non-Interval Detail)
	
		Required, unless an Exchange Date (DTM~514) is substituted for this code.
	
		DTM~151~20010131	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	151		Service Period End	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	

	Segment:	DTM Date/Time Reference (Exchange Date)
	Position:	020
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = PL (Non-Interval Detail)
	
		Required when a meter is exchanged and the meter agent does not change.
	
		Date Range in the first PTD is shown as:
   DTM~150~20010101
   DTM~514~20010114

Date Range in the second PTD is shown as:
   DTM~514~20010114
   DTM~151~20010128	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	514		Transferred	
	Exchange Date	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	

	Segment:	REF Reference Identification (Number of Dials)
	Position:	030
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	>1
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		Required for meters with dials	
		REF~IX~6.0
REF~IX~5.1
REF~IX~4.2

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	IX		Item Number	
	Number of Dials on the Meter displayed as the number of dials to the left of the decimal, a decimal point, and the number of dials to the right of the decimal.	
Used	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	Service Delivery Point ID	

	Segment:	REF Reference Identification (Meter Role)
	Position:	030
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	20
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		PTD = PL (Non-Interval Detail)
	
		Required
	
		REF~JH~A	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	JH		Tag	
	Meter Role	
Must Use	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
 	A		Additive 	
	This consumption must be added to the summarized total	
 	I		Ignore	
	This consumption did not contribute to the summarized total (do nothing)	
 	S		Subtractive 	
	This consumption must be subtracted from the summarized total	

	Segment:	REF Reference Identification (Meter Type)
	Position:	030
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	20
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		PTD = PL (Non-Interval Detail)

This segment is sent to indicate the type of usage that is reported in this PTD loop.	
		Required	
		REF~MT~K3015	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	MT		Meter Ticket Number	
	Meter Type	
Must Use	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	When REF01 is MT, the meter type is expressed as a five-character field.  The first two characters are the type of consumption, the last three characters are the metering interval reported by the metering agent.  Valid values can be a combination of the following values:

Type of Consumption

   K1  Kilowatt Demand (kW)
   K2  Kilovolt Amperes Reactive Demand (kVAR)
   K3  Kilovolt Amperes Reactive Hour (kVARH)
   K4  Kilovolt Amperes (kVA)
   KH  Kilowatt Hour (kWh)

Metering Interval Reported for Billing Purposes

  nnn  Number of minutes from 001 to 999
  DAY  Daily
  MON  Monthly
	
	For Example:
 
  KHMON  Kilowatt Hours Per Month
  K1015  Kilowatt Demand per 15 minute interval	

	Segment:	QTY Quantity
	Position:	110
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	1
	Purpose:	To specify quantity information
	Syntax Notes:	1	At least one of QTY02 or QTY04 is required.
		2	Only one of QTY02 or QTY04 may be present.
	Semantic Notes:	1	QTY04 is used when the quantity is non-numeric.
	Comments:
Notes:		PTD = PL (Non-Interval Detail)

There will be one QTY loop for each time of use  (i.e., one for On Peak kWh, one for Off Peak, kWh, one for Total kWh, etc.) 

Note: Quantity is the total measured consumption for the billable period including all billable adjustments applicable, e.g., transformer loss factor and the meter multiplier.  The quantity in the QTY02 has not been adjusted for any additive/Master Meter, subtractive/Master Meter or missing or abundance of consumption occurring in the PTD~PL when the PTD06 has a valid code.

MEA with an MEA07 = "51" (total)  is required. 

"KA" - Estimate must be used when reporting missing or abundance of consumption.
	
		Required	
		QTY~QD~1000	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	QTY01	673	Quantity Qualifier	M		ID 2/2	
	Code specifying the type of quantity	
	Note: There may be instances where the Quantity Qualifier could be AO or QD while the MEA01 is not AA (Meter reading-beginning actual/ending actual).	
 	AO		Verified Receipts	
	Verified as actual value	
 	KA		Estimated	
	Quantity is estimated
Required when reporting missing or abundance of consumption.	
 	QD		Quantity Delivered	
	Quantity is actual	
Must Use	QTY02	380	Quantity	X		R 1/15	
	Numeric value of quantity	
	Total Consumption / Max Demand	

	Segment:	MEA Measurements (Meter Reads)
	Position:	160
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	40
	Purpose:	To specify physical measurements or counts, including dimensions, tolerances, variances, and weights  (See Figures Appendix for example of use of C001)
	Syntax Notes:	1	At least one of MEA03 MEA05 MEA06 or MEA08 is required.
		2	If MEA05 is present, then MEA04 is required.
		3	If MEA06 is present, then MEA04 is required.
		4	If MEA07 is present, then at least one of MEA03 MEA05 or MEA06 is required.
		5	Only one of MEA08 or MEA03 may be present.
	Semantic Notes:	1	MEA04 defines the unit of measure for MEA03, MEA05, and MEA06.
	Comments:	1	When citing dimensional tolerances, any measurement requiring a sign (+ or -), or any measurement where a positive (+) value cannot be assumed, use MEA05 as the negative (-) value and MEA06 as the positive (+) value.
Notes:		PTD = PL (Non-Interval Detail)	
		Conditional - Required unless reporting Additive/Subtractive Metering Usage or Adjusted (missing or abundance) Consumption. (if the PTD06 equals "AI" , "AO","CD","DC","DM", or "MD")

MEA with an MEA07 = "51" (total) is required unless reporting Additive/Subtractive Metering Usage (the PTD06 equals "AI" or "AO","CD", "DC","DM", or "MD").  

		MEA~AA~PRQ~1000~KH~1000~1100~51	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	MEA01	737	Measurement Reference ID Code	O		ID 2/2	
	Code identifying the broad category to which a measurement applies	
 	AA		Meter reading-beginning actual/ending actual	
 	AE		Meter reading-beginning actual/ending estimated	
 	EA		Meter reading-beginning estimated/ending actual	
 	EE		Meter reading-beginning estimated/ending estimated	
Must Use	MEA02	738	Measurement Qualifier	O		ID 1/3	
	Code identifying a specific product or process characteristic to which a measurement applies	
 	PRQ		Product Reportable Quantity	
	Consumption	
Must Use	MEA03	739	Measurement Value	X		R 1/20	
	The value of the measurement	
	Total consumption after meter multiplier and transformer loss factor are applied.	
Must Use	MEA04	C001	Composite Unit of Measure	X			
	To identify a composite unit of measure  (See Figures Appendix for examples of use)	
	Please note that this is a composite data element, populate C00101.	
Must Use	C00101	355	Unit or Basis for Measurement Code	M		ID 2/2	
	Code specifying the units in which a value is being expressed, or manner in which a measurement has been taken	
 	K1		Kilowatt Demand	
	kW	
 	K2		Kilovolt Amperes Reactive Demand	
	kVAR	
 	K3		Kilovolt Amperes Reactive Hour	
	kVARH	
 	K4		Kilovolt Amperes	
	kVA	
 	KH		Kilowatt Hour	
	kWh	
Dep	MEA05	740	Range Minimum	X		R 1/20	
	The value specifying the minimum of the measurement range	
	The Beginning read is required when C00101, element 355 Unit of Measure is equal to
 "K3" - kVARH (Kilovolt Amperes Reactive Hour),
 "K4" - kVA (Kilovolt Amperes) 
 "KH" - kWh (Kilowatt Hour).

The Beginning read is not used for
 "K1" - kW (Kilowatt Demand)
 "K2" - kVAR (Kilovolt Amperes Reactive Demand).	
	 	
Must Use	MEA06	741	Range Maximum	X		R 1/20	
	The value specifying the maximum of the measurement range	
	Ending reading when C00101, element 355 Unit of Measure is equal to 
"K3" - kVARH (Kilovolt Amperes Reactive Hour)
"K4" - kVA (Kilovolt Amperes)
"KH" - kWh (Kilowatt Hour)

Single reading when
"K1" - kW (Kilowatt Demand)
"K2" - kVAR (Kilovolt Amperes Reactive Demand)	
Must Use	MEA07	935	Measurement Significance Code	O		ID 2/2	
	Code used to benchmark, qualify or further define a measurement value	
 	41		Off Peak	
 	42		On Peak	
 	43		Intermediate	
	Mid-Peak	
 	51		Total	
	Totalizer/Total/Max (Demand)	
 	71		Low	
	Summer Super On-Peak	

	Segment:	MEA Measurements (Transformer Loss Factor)
	Position:	160
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	40
	Purpose:	To specify physical measurements or counts, including dimensions, tolerances, variances, and weights  (See Figures Appendix for example of use of C001)
	Syntax Notes:	1	At least one of MEA03 MEA05 MEA06 or MEA08 is required.
		2	If MEA05 is present, then MEA04 is required.
		3	If MEA06 is present, then MEA04 is required.
		4	If MEA07 is present, then at least one of MEA03 MEA05 or MEA06 is required.
		5	Only one of MEA08 or MEA03 may be present.
	Semantic Notes:	1	MEA04 defines the unit of measure for MEA03, MEA05, and MEA06.
	Comments:	1	When citing dimensional tolerances, any measurement requiring a sign (+ or -), or any measurement where a positive (+) value cannot be assumed, use MEA05 as the negative (-) value and MEA06 as the positive (+) value.
Notes:		PTD = PL (Non-Interval Detail)
	
		Required when the transformer loss is not measured by the meter

"Where the delivery point is prior to the transformation such that the customer is responsible for losses and the meter is after the transformer and therefore does not record losses, the transformer loss factor will be greater that unity.  E.g.  1.006, to reflect a positive adjustment to the meter readiness.  Where the delivery point is after the transformation such that the customer is not responsible for transformer losses, and the meter is prior to the transformer and therefore does reflect transformer losses, the transformer loss factor will be less that unity.  E.g.  0.995, to reflect a negative adjustment to the meter readings."
	
		The value in the field will always be a positive value, for example:
MEA~~CO~1.015 (format when the factor is positive)
MEA~~CO~.985 (format when the factor is negative)

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	MEA02	738	Measurement Qualifier	O		ID 1/3	
	Code identifying a specific product or process characteristic to which a measurement applies	
 	CO		Core Loss	
	Transformer Loss Factor	
Must Use	MEA03	739	Measurement Value	X		R 1/20	
	The value of the measurement	
	Transformer Loss Factor	

	Segment:	MEA Measurements (Meter Multiplier)
	Position:	160
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	40
	Purpose:	To specify physical measurements or counts, including dimensions, tolerances, variances, and weights  (See Figures Appendix for example of use of C001)
	Syntax Notes:	1	At least one of MEA03 MEA05 MEA06 or MEA08 is required.
		2	If MEA05 is present, then MEA04 is required.
		3	If MEA06 is present, then MEA04 is required.
		4	If MEA07 is present, then at least one of MEA03 MEA05 or MEA06 is required.
		5	Only one of MEA08 or MEA03 may be present.
	Semantic Notes:	1	MEA04 defines the unit of measure for MEA03, MEA05, and MEA06.
	Comments:	1	When citing dimensional tolerances, any measurement requiring a sign (+ or -), or any measurement where a positive (+) value cannot be assumed, use MEA05 as the negative (-) value and MEA06 as the positive (+) value.
Notes:		PTD = PL (Non-Interval Detail)

If no meter multiplier, then populate with "1"

Note:  Format of the multiplier could be in the form of a fraction (e.g. 48.78432)
	
		Required
	
		MEA~~MU~1	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	MEA02	738	Measurement Qualifier	O		ID 1/3	
	Code identifying a specific product or process characteristic to which a measurement applies	
 	MU		Multiplier	
	Meter Multiplier

(Ending Reading - Beginning Reading) * Meter Multiplier = Billed Usage	
Must Use	MEA03	739	Measurement Value	X		R 1/20	
	The value of the measurement	
	Meter Multiplier	

	Segment:	MEA Measurements (Power Factor)
	Position:	160
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	40
	Purpose:	To specify physical measurements or counts, including dimensions, tolerances, variances, and weights  (See Figures Appendix for example of use of C001)
	Syntax Notes:	1	At least one of MEA03 MEA05 MEA06 or MEA08 is required.
		2	If MEA05 is present, then MEA04 is required.
		3	If MEA06 is present, then MEA04 is required.
		4	If MEA07 is present, then at least one of MEA03 MEA05 or MEA06 is required.
		5	Only one of MEA08 or MEA03 may be present.
	Semantic Notes:	1	MEA04 defines the unit of measure for MEA03, MEA05, and MEA06.
	Comments:	1	When citing dimensional tolerances, any measurement requiring a sign (+ or -), or any measurement where a positive (+) value cannot be assumed, use MEA05 as the negative (-) value and MEA06 as the positive (+) value.
Notes:		PTD = PL (Non-Interval Detail)

Required if measured
	
		MEA~~ZA~.95	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	MEA02	738	Measurement Qualifier	O		ID 1/3	
	Code identifying a specific product or process characteristic to which a measurement applies	
 	ZA		Power Factor	
	Relationship between watts and volt - amperes necessary to supply electric load	
Must Use	MEA03	739	Measurement Value	X		R 1/20	
	The value of the measurement	
	Power Factor	

	Segment:	PTD Product Transfer and Resale Detail (Unmetered Services)
	Position:	010
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Mandatory
	Max Use:	1
	Purpose:	To indicate the start of detail information relating to the transfer/resale of a product and provide identifying data
	Syntax Notes:	1	If either PTD02 or PTD03 is present, then the other is required.
		2	If either PTD04 or PTD05 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = BD (Unmetered Services)

One PTD loop is required per device type per customer account id.  Total consumption for all unmetered services is at the unmetered device detail level.  One loop is required for each unmetered device type per each unique wattage and/or lumen reported.  Even though some consumption may be estimated, the consumption is reported as actual quantity delivered for unmetered services.  The detail is required for Unmetered Services.
	
		One PTD loop is required for each unmetered service type.	
		PTD~BD	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	PTD01	521	Product Transfer Type Code	M		ID 2/2	
	Code identifying the type of product transfer	
 	BD		Issue - Other Department	
	Unmetered Services Detail	

	Segment:	DTM Date/Time Reference (Service Period Start)
	Position:	020
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = BD (Unmetered Services)
	
		Required

The DTM*150 (Service Period Begin Date) for Month 2 must equal the DTM*151 (Service Period End Date) for Month 1, otherwise a gap in data exists.  See below example:
          Service Period Begin Date          Service Period End Date
Month 1           DTM~150~20010501          DTM~151~20010601
Month 2          DTM~150~20010601          DTM~151~20010701
	
		DTM~150~20010101	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	150		Service Period Start	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	

	Segment:	DTM Date/Time Reference (Service Period End)
	Position:	020
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = BD (Unmetered Services)
	
		Required

The DTM*150 (Service Period Begin Date) for Month 2 must equal the DTM*151 (Service Period End Date) for Month 1, otherwise a gap in data exists.  See below example:
          Service Period Begin Date          Service Period End Date
Month 1           DTM~150~20010501          DTM~151~20010601
Month 2          DTM~150~20010601          DTM~151~20010701

		DTM~151~20010131	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	151		Service Period End	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	

	Segment:	REF Reference Identification (Unmetered Service Type)
	Position:	030
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	20
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		This segment is used to provide additional information to the CR for the specified Unmetered Service.  It describes the type of device which this measurement loop references and can include additional text information which may be useful to the CR (i.e., a specific wattage of a light, additional text information for further clarification, etc.)

PTD = BD (Unmetered Services)
	
		Required if there are unmetered services on the account
	
		REF~PRT~MV~750
REF~PRT~SD~400 Company Owned
REF~PRT~SD~400 Customer Owned
REF~PRT~MV~Third party maintained facilities

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	PRT		Product Type	
	Defined Unmetered Service Type	
Must Use	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	RBC - see governing documents for valid unmetered type codes.	
 	AN		Antenna	
 	AR		Argon	
 	BB		Bill Boards	
 	BS		Bus Shelters	
 	CU		Cat Unit	
 	ED		Electronic Device	
 	FL		Fluorescent	
 	HA		Historical/Antique	
 	IN		Incandescent	
 	LV		Levys	
 	MH		Metal Halide	
 	MV		Mercury Vapor	
 	OT		Other Un-Metered	
 	PA		Power Analog node	
 	PB		Phone Booth	
 	PO		Phone Outlet	
 	PS		Pump Station	
 	RR		Rail Road Crossings	
 	SD		Sodium	
 	TL		Traffic Lights	
 	TR		Tranceiver	
 	WM		Wallpacked Mercury Vapor	
 	WS		Warning Sirens	
Dep	REF03	352	Description	X		AN 1/80	
	A free-form description to clarify the related data elements and their content	
	Used to provide additional clarification information to the non-billing party for the Unmetered Service when necessary.  When applicable, used to provide the specific wattage/lumens for a light.
	
	This free-form text can not contain  any characters that may be used as element delimiters, sub-element delimiters, segment terminators, or field separators(This includes: asterisk *, pipes |, tabs, linefeeds, carets ^, angle brackets < >, and tildes ~).	

	Segment:	QTY Quantity
	Position:	110
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	1
	Purpose:	To specify quantity information
	Syntax Notes:	1	At least one of QTY02 or QTY04 is required.
		2	Only one of QTY02 or QTY04 may be present.
	Semantic Notes:	1	QTY04 is used when the quantity is non-numeric.
	Comments:
Notes:		PTD = BD (Unmetered Services)	
		One QTY Loop is required for each consumption quantity per device.

Note: The billable quantity is the total unmetered consumption per device type for the billable period.  There is no PTD06 = "AI","A0","CD","DC","DM" or "MD" Adjusted Consumption in this loop.  Billable quantity in the 867-03 may not match the invoiced quantity in the 810_02 because of TDSP tariff adjustments to the 810_02 data.	
		QTY~QD~2000~EA^^20^KH^^100	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	QTY01	673	Quantity Qualifier	M		ID 2/2	
	Code specifying the type of quantity	
 	QD		Quantity Delivered	
Must Use	QTY02	380	Quantity	X		R 1/15	
	Numeric value of quantity	
	Total consumption of device type.	
Must Use	QTY03	C001	Composite Unit of Measure	O			
	To identify a composite unit of measure  (See Figures Appendix for examples of use)	
	Note this is a composite data element, populate C00101	
Must Use	C00101	355	Unit or Basis for Measurement Code	M		ID 2/2	
	Code specifying the units in which a value is being expressed, or manner in which a measurement has been taken	
 	EA		Each	
Must Use	C00103	649	Multiplier	O		R 1/10	
	Value to be used as a multiplier to obtain a new value	
	Number of unmetered devices for this specific Unmetered Service Type (as defined in the REF~PRT segment).	
Must Use	C00104	355	Unit or Basis for Measurement Code	O		ID 2/2	
	Code specifying the units in which a value is being expressed, or manner in which a measurement has been taken	
 	KH		Kilowatt Hour	
Must Use	C00106	649	Multiplier	O		R 1/10	
	Value to be used as a multiplier to obtain a new value	
	This represents the consumption quantity per device	

	Segment:	PTD Product Transfer and Resale Detail (Interval Summary)
	Position:	010
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Mandatory
	Max Use:	1
	Purpose:	To indicate the start of detail information relating to the transfer/resale of a product and provide identifying data
	Syntax Notes:	1	If either PTD02 or PTD03 is present, then the other is required.
		2	If either PTD04 or PTD05 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = BO (Interval Summary)
	
		One PTD~BO loop is required for each meter for each unit of measure.  The PTD~BO reports monthly interval consumption at each meter.  There will be separate PTD~BO loops to reflect summed adjusted consumption.

Individual intervals are not reported in the PTD~BO loop.  The PTD~BO loop will never report KW or KVAR.  

For Additive/Subtractive Metering Only:
This loop is also used for Additive/Subtractive Metering when the Master Meter is on one SDID  and the additive and/or subtractive meters are on SDID that are different than the master Meter.   All additive and subtractive usage is summed. It is possible to receive two additive/subtractive loops - one with summed additive usage and one with summed subtractive usage.  When reporting usage for the additive/Master and/or subtractive/Master usage, the meter number is not provided in the PTD04 and PTD05.  The type of Master/Subtractive and/or Master/ Additive usage must be provided in the PTD06 by using code "AI" or code "AO".   Distribution Companies provide for the Master/Subtractive or Master/Additive net intervals in the PTD~PP when the PTD~BO element  PTD06  equals   "AI" or "AO".   No netted usage is reported in this Loop.  The receiver must net the PTD~BO Loops to determine Master Meter usage.

Missing or Abundance of Consumption:
Not reported for Interval Meters.
	
		PTD~BO~~~MG~1234568MG
PTD~BO~~~~~AI (used to report Additive/Master metering usage)
PTD~BO~~~~~AO (used to report Subtractive/Master metering usage)	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	PTD01	521	Product Transfer Type Code	M		ID 2/2	
	Code identifying the type of product transfer	
 	BO		Designated Items	
	Consumption across intervals and across the same unit of measure summarized at the meter level	
Dep	PTD04	128	Reference Identification Qualifier	X		ID 2/3	
	Code qualifying the Reference Identification	
 	MG		Meter Number	
	Not used if the PTD06 = "AO" or "AI"	
Dep	PTD05	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	Meter Number

Meter numbers will contain only uppercase letters (A to Z) and digits (0 to 9).  Note that punctuation (spaces, dashes, etc.) must be excluded, and significant leading and trailing zeros that are part of the meter number must be present.

Not used if the PTD06 = "AO" or "AI".
	
Used	PTD06	486	Product Transfer Movement Type Code	O		ID 2/2	
	To indicate the type of product transfer movement	
	This field is only used when reporting the type of Master/Additive or Master/Subtractive usage.  This indicates to the receiver that they will find the netted interval usage for the Master Meter the PTD~PP.	
 	AI		Adjustment In	
	Additive Metering

Additive Usage for Additive meters off the master meter where a different SDID has been assigned to the master and/or all applicable additive meters.  When the PTD06 equals "AI", the REF~JH equals "A".	
 	AO		Adjustment Out	
	Subtractive Metering

Subtractive Usage for Subtract meters off the master meter where a different SDID has been assigned to the master and/or all applicable subtractive meters.  .  When the PTD06 equals "AO", the REF~JH equals "S".	

	Segment:	DTM Date/Time Reference (Service Period Start)
	Position:	020
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = BO (Interval Summary)
	
		Required, unless an Exchange Date (DTM~514) is substituted for this code.
	
		DTM~150~20010101	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	150		Service Period Start	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	

	Segment:	DTM Date/Time Reference (Service Period End)
	Position:	020
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = BO (Interval Summary)
	
		Required, unless an Exchange Date (DTM~514) is substituted for this code.
	
		DTM~151~20010131	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	151		Service Period End	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	

	Segment:	DTM Date/Time Reference (Exchange Date)
	Position:	020
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = BO (Interval Summary)
	
		Required when a meter is exchanged and the meter agent does not change.
	
		Date Range in the first PTD is shown as:
   DTM~150~19990201
   DTM~514~19990214

Date Range in the second PTD is shown as:
   DTM~514~19990214
   DTM~151~19990228	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	514		Transferred	
	Exchange Date	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	

	Segment:	REF Reference Identification (Meter Role)
	Position:	030
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	20
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		PTD = BO (Interval Summary)	
		Required
	
		REF~JH~A	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	JH		Tag	
	Meter Role	
Must Use	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
 	A		Additive 	
	This consumption contributed to the summarized total (do nothing)	
 	I		Ignore	
	This consumption did not contribute to the summarized total (do nothing)	
 	S		Subtractive 	
	This consumption must be subtracted from the summarized total	

	Segment:	REF Reference Identification (Meter Type)
	Position:	030
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	20
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		PTD = BO (Interval Summary)

This segment is sent primarily to indicate the type of usage that is reported in this PTD loop.  There will be one PTD loop for each unit of measure.
	
		Required
	
		REF~MT~KHMON	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	MT		Meter Ticket Number	
	Meter Type	
Must Use	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	     When REF01 is MT, the meter type is expressed as a five-character field.  The first two characters are the type of consumption, the last three characters are the metering interval reported by the metering agent.  Valid values can be a combination of the following values:

Type of Consumption

   K1  Kilowatt Demand (kW)   
                (NOT USED FOR INTERVAL METERS)
   K2  Kilovolt Amperes Reactive Demand (kVAR)  
                (NOT USED FOR INTERVAL METERS)
   K3  Kilovolt Amperes Reactive Hour (kVARH)
   K4  Kilovolt Amperes (kVA)
                 NOT USED FOR INTERVAL METERS

   KH  Kilowatt Hour (kWh)

Metering Interval Reported for Billing Purposes

  nnn  Number of minutes from 001 to 999
  DAY  Daily
  MON  Monthly

For Example:
 
  KHMON  Kilowatt Hours Per Month
  K1015  Kilowatt Demand per 15 minute interval	

	Segment:	QTY Quantity
	Position:	110
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	1
	Purpose:	To specify quantity information
	Syntax Notes:	1	At least one of QTY02 or QTY04 is required.
		2	Only one of QTY02 or QTY04 may be present.
	Semantic Notes:	1	QTY04 is used when the quantity is non-numeric.
	Comments:
Notes:		PTD = BO (Interval Summary)	
		Required

Note: The quantity is the total measured consumption for the billable period including all billable adjustments applicable, e.g., transformer loss factor and the meter multiplier.  The quantity in the QTY02 has not been adjusted for any master/additive/ subtractive meter usage.

Quantity is sent with a minimum of two digits and a maximum of four digits to the right of the decimal point, e.g., 525.15; 567.1375, etc., while adhering to the ANSI rules for providing Real numbers.  For instance, if the quantity reported is:
525                     then the QTY02 is reported as                525
525.1275            then the QTY02 is reported as                525.1275
525.12                then the QTY02 is reported as                525.12
525.10                then the QTY02 is reported as                525.1
0                         then the QTY02 is reported as                0
Leading zeros are suppressed and trailing zeros are truncated.  Please refer to ANSI ASC X12 Version 004010 for further information on ANSI data elements, segments and loop usage and requirements.
	
		QTY~QD~746	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	QTY01	673	Quantity Qualifier	M		ID 2/2	
	Code specifying the type of quantity	
 	KA		Estimated	
	Quantity is estimated	
 	QD		Quantity Delivered	
	Quantity is actual	
Must Use	QTY02	380	Quantity	X		R 1/15	
	Numeric value of quantity	

	Segment:	MEA Measurements (Meter Reads)
	Position:	160
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	40
	Purpose:	To specify physical measurements or counts, including dimensions, tolerances, variances, and weights  (See Figures Appendix for example of use of C001)
	Syntax Notes:	1	At least one of MEA03 MEA05 MEA06 or MEA08 is required.
		2	If MEA05 is present, then MEA04 is required.
		3	If MEA06 is present, then MEA04 is required.
		4	If MEA07 is present, then at least one of MEA03 MEA05 or MEA06 is required.
		5	Only one of MEA08 or MEA03 may be present.
	Semantic Notes:	1	MEA04 defines the unit of measure for MEA03, MEA05, and MEA06.
	Comments:	1	When citing dimensional tolerances, any measurement requiring a sign (+ or -), or any measurement where a positive (+) value cannot be assumed, use MEA05 as the negative (-) value and MEA06 as the positive (+) value.
Notes:		PTD = BO (Interval Summary)
	
		Conditional - Required unless reporting Additive/Subtractive Metering Usage. (if the PTD06 equals "AI" or "AO").

MEA with an MEA07 = "51" (total) is required unless reporting Additive/Subtractive Metering Usage (the PTD06  equals "AI" or "AO").  
	
		MEA~AF~~~KH~9500~10231~51	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	MEA01	737	Measurement Reference ID Code	O		ID 2/2	
	Code identifying the broad category to which a measurement applies	
 	AF		Actual Total	
Must Use	MEA04	C001	Composite Unit of Measure	X			
	To identify a composite unit of measure  (See Figures Appendix for examples of use)	
	This is a composite data element, please populate C00101	
Must Use	C00101	355	Unit or Basis for Measurement Code	M		ID 2/2	
	Code specifying the units in which a value is being expressed, or manner in which a measurement has been taken	
 	K3		Kilovolt Amperes Reactive Hour	
	kVARH	
 	KH		Kilowatt Hour	
	kWh	
Dep	MEA05	740	Range Minimum	X		R 1/20	
	The value specifying the minimum of the measurement range	
	The Beginning Read.	
	Required when C00101 equals  "KH" - kWh (Kilowatt Hour).  
	
Must Use	MEA06	741	Range Maximum	X		R 1/20	
	The value specifying the maximum of the measurement range	
	Ending Reading. 	
Must Use	MEA07	935	Measurement Significance Code	O		ID 2/2	
	Code used to benchmark, qualify or further define a measurement value	
 	51		Total	
	Totalizer/Total/Max (Demand)	

	Segment:	MEA Measurements (Transformer Loss Factor)
	Position:	160
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	40
	Purpose:	To specify physical measurements or counts, including dimensions, tolerances, variances, and weights  (See Figures Appendix for example of use of C001)
	Syntax Notes:	1	At least one of MEA03 MEA05 MEA06 or MEA08 is required.
		2	If MEA05 is present, then MEA04 is required.
		3	If MEA06 is present, then MEA04 is required.
		4	If MEA07 is present, then at least one of MEA03 MEA05 or MEA06 is required.
		5	Only one of MEA08 or MEA03 may be present.
	Semantic Notes:	1	MEA04 defines the unit of measure for MEA03, MEA05, and MEA06.
	Comments:	1	When citing dimensional tolerances, any measurement requiring a sign (+ or -), or any measurement where a positive (+) value cannot be assumed, use MEA05 as the negative (-) value and MEA06 as the positive (+) value.
Notes:		PTD = BO (Interval Summary)
	
		Required when the transformer loss is not measured by the meter

"Where the delivery point is prior to the transformation such that the customer is responsible for losses and the meter is after the transformer and therefore does not record losses, the transformer loss factor will be greater that unity.  E.g.  1.006, to reflect a positive adjustment to the meter readiness.  Where the delivery point is after the transformation such that the customer is not responsible for transformer losses, and the meter is prior to the transformer and therefore does reflect transformer losses, the transformer loss factor will be less that unity.  E.g.  0.995, to reflect a negative adjustment to the meter readings."
	
		The value in the field will always be a positive value, for example:
MEA~~CO~1.015 (format when the factor is positive)
MEA~~CO~.985 (format when the factor is negative)

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	MEA02	738	Measurement Qualifier	O		ID 1/3	
	Code identifying a specific product or process characteristic to which a measurement applies	
 	CO		Core Loss	
	Transformer Loss Factor	
Must Use	MEA03	739	Measurement Value	X		R 1/20	
	The value of the measurement	
	Transformer Loss Factor	

	Segment:	MEA Measurements (Meter Multiplier)
	Position:	160
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	40
	Purpose:	To specify physical measurements or counts, including dimensions, tolerances, variances, and weights  (See Figures Appendix for example of use of C001)
	Syntax Notes:	1	At least one of MEA03 MEA05 MEA06 or MEA08 is required.
		2	If MEA05 is present, then MEA04 is required.
		3	If MEA06 is present, then MEA04 is required.
		4	If MEA07 is present, then at least one of MEA03 MEA05 or MEA06 is required.
		5	Only one of MEA08 or MEA03 may be present.
	Semantic Notes:	1	MEA04 defines the unit of measure for MEA03, MEA05, and MEA06.
	Comments:	1	When citing dimensional tolerances, any measurement requiring a sign (+ or -), or any measurement where a positive (+) value cannot be assumed, use MEA05 as the negative (-) value and MEA06 as the positive (+) value.
Notes:		PTD = BO (Interval Summary)
	
		Required for all IDR Meters when meter readings are reported.  Not provided for additive/subtractive meters when they are on a different SDID's than the Master Meter because meter readings are not reported.
	
		MEA~~MU~20000000.12345	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	MEA02	738	Measurement Qualifier	O		ID 1/3	
	Code identifying a specific product or process characteristic to which a measurement applies	
 	MU		Multiplier	
	Meter Multiplier

(Ending Reading - Beginning Reading) * Meter Multiplier = Consumption reported in this PTD~BO Loop (within VEE tolerances).	
Must Use	MEA03	739	Measurement Value	X		R 1/20	
	The value of the measurement	
	Meter Multiplier

Meter Multipliers for IDR Meters can be quite large.  Format allows for eight digits to the left of the decimal and five digits to the right of the decimal, e.g., 9999999.99999.	

	Segment:	MEA Measurements (Power Factor)
	Position:	160
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	40
	Purpose:	To specify physical measurements or counts, including dimensions, tolerances, variances, and weights  (See Figures Appendix for example of use of C001)
	Syntax Notes:	1	At least one of MEA03 MEA05 MEA06 or MEA08 is required.
		2	If MEA05 is present, then MEA04 is required.
		3	If MEA06 is present, then MEA04 is required.
		4	If MEA07 is present, then at least one of MEA03 MEA05 or MEA06 is required.
		5	Only one of MEA08 or MEA03 may be present.
	Semantic Notes:	1	MEA04 defines the unit of measure for MEA03, MEA05, and MEA06.
	Comments:	1	When citing dimensional tolerances, any measurement requiring a sign (+ or -), or any measurement where a positive (+) value cannot be assumed, use MEA05 as the negative (-) value and MEA06 as the positive (+) value.
Notes:		PTD = BO (Interval Summary)
	
		Required if measured
	
		MEA~~ZA~.95	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	MEA02	738	Measurement Qualifier	O		ID 1/3	
	Code identifying a specific product or process characteristic to which a measurement applies	
 	ZA		Power Factor	
	Relationship between watts and volt - amperes necessary to supply electric load	
Must Use	MEA03	739	Measurement Value	X		R 1/20	
	The value of the measurement	
	Power Factor	

	Segment:	PTD Product Transfer and Resale Detail (Interval Detail)
	Position:	010
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Mandatory
	Max Use:	1
	Purpose:	To indicate the start of detail information relating to the transfer/resale of a product and provide identifying data
	Syntax Notes:	1	If either PTD02 or PTD03 is present, then the other is required.
		2	If either PTD04 or PTD05 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = PM (Interval Detail)	
		One PTD~PM loop is required for each meter channel for each unit of measure.  Demand is not reported in the PTD~PM loop.  This is the lowest level of detail.  

Distribution Companies must report 15-minute intervals in the PTD~PM.  ??

		PTD~PM~~~MG~1234568MG	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	PTD01	521	Product Transfer Type Code	M		ID 2/2	
	Code identifying the type of product transfer	
 	PM		Physical Meter Information	
	Interval Detail	
Must Use	PTD04	128	Reference Identification Qualifier	X		ID 2/3	
	Code qualifying the Reference Identification	
 	MG		Meter Number	
Must Use	PTD05	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	Meter Number

Meter numbers will contain only uppercase letters (A to Z) and digits (0 to 9).  Note that punctuation (spaces, dashes, etc.) must be excluded, and significant leading and trailing zeros that are part of the meter number must be present.

	Segment:	DTM Date/Time Reference (Service Period Start)
	Position:	020
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = PM (Interval Detail)
	
		Required, unless an Exchange Date (DTM~514) is substituted for this code.
	
		DTM~150~20010101	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	150		Service Period Start	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	

	Segment:	DTM Date/Time Reference (Service Period End)
	Position:	020
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = PM (Interval Detail)
	
		Required, unless an Exchange Date (DTM~514) is substituted for this code.
	
		DTM~151~20010131	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	151		Service Period End	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	

	Segment:	DTM Date/Time Reference (Exchange Date)
	Position:	020
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = PM (Interval Detail)
	
		Required when a meter is exchanged and the meter agent does not change.
	
		Date Range in the first PTD is shown as:
   DTM~150~20010101
   DTM~514~20010114~1200

Date Range in the second PTD is shown as:
   DTM~514~20010114~1200
   DTM~151~20010128	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	514		Transferred	
	Exchange Date	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	
Must Use	DTM03	337	Time	X		TM 4/8	
	Time expressed in 24-hour clock time as follows: HHMM, or HHMMSS, or HHMMSSD, or HHMMSSDD, where H = hours (00-23), M = minutes (00-59), S = integer seconds (00-59) and DD = decimal seconds; decimal seconds are expressed as follows: D = tenths (0-9) and DD = hundredths (00-99)	
	HHMM, where H = Hours (00 to 23) and M = Minutes (00 to 59) in Central Prevailing Time (CT).  For this transaction, since X12 does not allow 2400 for time, 2359 will be used to indicate midnight.  For example, midnight between October 15th and October 16th will be reflected as 2359 of October 15th.	

	Segment:	REF Reference Identification (Channel Number)
	Position:	030
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	20
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		PTD = PM (Interval Detail)	
		Required	
		REF~6W~2	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	6W		Sequence Number	
	Channel Number	
Must Use	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	Channel Number	

	Segment:	REF Reference Identification (Meter Type)
	Position:	030
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	20
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		PTD = PM (Interval Detail)	
		This segment is sent to indicate the type of usage that is reported in this PTD loop.

Required	
		REF~MT~KHMON	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	MT		Meter Ticket Number	
	Meter Type	
Must Use	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
	     When REF01 is MT, the meter type is expressed as a five-character field.  The first two characters are the type of consumption, the last three characters are the metering interval reported by the metering agent.  Valid values can be a combination of the following values:

Type of Consumption

   K1  Kilowatt Demand (kW)
                NOT USED
   K2  Kilovolt Amperes Reactive Demand (kVAR)
                NOT USED
   K3  Kilovolt Amperes Reactive Hour (kVARH)
   K4  Kilovolt Amperes (kVA)
                NOT USED

   KH  Kilowatt Hour (kWh)

Metering Interval Reported for Billing Purposes

  nnn  Number of minutes from 001 to 999
  DAY  Daily
  MON  Monthly

For Example:
 
  KHMON  Kilowatt Hours Per Month
  K1015  Kilowatt Demand per 15 minute interval	

	Segment:	REF Reference Identification (Meter Role)
	Position:	030
	Loop:	PTD        Mandatory
	Level:	Detail
	Usage:	Optional
	Max Use:	20
	Purpose:	To specify identifying information
	Syntax Notes:	1	At least one of REF02 or REF03 is required.
		2	If either C04003 or C04004 is present, then the other is required.
		3	If either C04005 or C04006 is present, then the other is required.
	Semantic Notes:	1	REF04 contains data relating to the value cited in REF02.
	Comments:
Notes:		PTD = PM (Interval Detail)
	
		Required
	
		REF~JH~A	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	REF01	128	Reference Identification Qualifier	M		ID 2/3	
	Code qualifying the Reference Identification	
 	JH		Tag	
	Meter Role	
Must Use	REF02	127	Reference Identification	X		AN 1/30	
	Reference information as defined for a particular Transaction Set or as specified by the Reference Identification Qualifier	
 	A		Additive 	
	This consumption must be added to the summarized total 	
 	I		Ignore	
	This consumption did not contribute to the summarized total (do nothing)	
 	S		Subtractive 	
	This consumption must be subtracted from the summarized total	

	Segment:	QTY Quantity
	Position:	110
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	1
	Purpose:	To specify quantity information
	Syntax Notes:	1	At least one of QTY02 or QTY04 is required.
		2	Only one of QTY02 or QTY04 may be present.
	Semantic Notes:	1	QTY04 is used when the quantity is non-numeric.
	Comments:
Notes:		PTD = PM (Interval Detail)	
		Note: Quantity is the total measured interval consumption for the billable period including all billable adjustments applicable, e.g., transformer loss factor and the meter multiplier.  The quantity in the QTY02 has not been adjusted for any additive and/or subtractive usage.

Quantity is sent with a minimum of two digits and a maximum of four digits to the right of the decimal point, e.g., 525.15; 567.1375, etc., while adhering to the ANSI rules for providing Real numbers.  For instance, if the quantity reported is:
525                     then the QTY02 is reported as                525
525.1275            then the QTY02 is reported as                525.1275
525.12                then the QTY02 is reported as                525.12
525.10                then the QTY02 is reported as                525.1
0                         then the QTY02 is reported as                0
Leading zeros are suppressed and trailing zeros are truncated.  Please refer to ANSI ASC X12 Version 004010 for further information on ANSI data elements, segments and loop usage and requirements.

		QTY~QD~22348	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	QTY01	673	Quantity Qualifier	M		ID 2/2	
	Code specifying the type of quantity	
 	KA		Estimated	
	Quantity is estimated	
 	QD		Quantity Delivered	
	Quantity is actual	
Must Use	QTY02	380	Quantity	X		R 1/15	
	Numeric value of quantity	

	Segment:	DTM Date/Time Reference (Interval End Time)
	Position:	210
	Loop:	QTY        Optional
	Level:	Detail
	Usage:	Optional
	Max Use:	10
	Purpose:	To specify pertinent dates and times
	Syntax Notes:	1	At least one of DTM02 DTM03 or DTM05 is required.
		2	If DTM04 is present, then DTM03 is required.
		3	If either DTM05 or DTM06 is present, then the other is required.
	Semantic Notes:
	Comments:
Notes:		PTD = PM (Interval Detail)
	
		Required
	
		DTM~194~20010115~1500	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	DTM01	374	Date/Time Qualifier	M		ID 3/3	
	Code specifying type of date or time, or both date and time	
 	194		Period End	
	The date/time of the end of the interval	
Must Use	DTM02	373	Date	X		DT 8/8	
	Date expressed as CCYYMMDD	
Must Use	DTM03	337	Time	X		TM 4/8	
	Time expressed in 24-hour clock time as follows: HHMM, or HHMMSS, or HHMMSSD, or HHMMSSDD, where H = hours (00-23), M = minutes (00-59), S = integer seconds (00-59) and DD = decimal seconds; decimal seconds are expressed as follows: D = tenths (0-9) and DD = hundredths (00-99)	
	HHMM, where H = Hours (00 to 23) and M = Minutes (00 to 59) in Central Prevailing Time (CT).  For this transaction, since X12 does not allow 2400 for time, 2359 will be used to indicate midnight.  For example, midnight between October 15th and October 16th will be reflected as 2359 of October 15th.	

	Segment:	SE Transaction Set Trailer
	Position:	030
	Loop:
	Level:	Summary
	Usage:	Mandatory
	Max Use:	1
	Purpose:	To indicate the end of the transaction set and provide the count of the transmitted segments (including the beginning (ST) and ending (SE) segments)
	Syntax Notes:
	Semantic Notes:
	Comments:	1	SE is the last segment of each transaction set.
Notes:		Required
	
		SE~42~000000001	

Data Element Summary
	Ref.	Data	
	Des.	Element	Name	Attributes
Must Use	SE01	96	Number of Included Segments	M		N0 1/10	
	Total number of segments included in a transaction set including ST and SE segments	
Must Use	SE02	329	Transaction Set Control Number	M		AN 4/9	
	Identifying control number that must be unique within the transaction set functional group assigned by the originator for a transaction set