Parking Lot Issue 7 Considerations

Curtailments of tags that come in after the event is called:

When a curtailment event has been called, no new tags that would contribute positive flows to the congested transmission element should be held. Such tags would be accepted but immediately cut.

A tag that is determined to be a “Restricted Tag“ is identified as a “Post-USF Tag“ in the webECC USF event as follows:

* a new transaction with a Transfer Distribution Factor (TDF) on the Qualified Transfer Path equal to or greater than 10 percent in the qualified direction (this new tag is immediately curtailed to zero) or
* the increase in a Pre-Event Schedule, with a TDF on the Qualified Transfer Path equal to or greater than 10 percent in the qualified direction.