Scoping document

2019 API 3c item 7

Statement: Modification of the SR profile independent of the DNR profile

Scope:

1. What
   1. Modify SR request will be used during the life of the DNR
   2. SR request is explicitly linked to a DNR (?)
   3. Any templates for the SR request we should have the DNR reference/Resource name.
   4. Similarly to an e-Tag entry
   5. Profile for the SR should be under the limit of the DNR (?)
      1. Some implementations require that the SR do not exceed DNR profiles while others require flexibility for SR to exceed the DNR profiles.
   6. Need to handle partial SR of a DNR
2. When
   1. What are the timing requirements
   2. Table 105-A NITS Request Timing Requirements
3. Who
   1. Transmission Customer
   2. Transmission Provider on behalf of the Transmission Customer
4. How
   1. Make a new SR request (modify SR request) and to use the existing SR and DNR template structures for modifications.
   2. If a DNR is partially terminated then the SR will be affect by
      1. the amount of the partial termination only by the amount of the termination minus the SR affected
      2. a modify SR request will not be needed
      3. a redesignation of the DNR will bring SR back to the original if affected
   3. Will the NITS transition states still apply with this SR request